# Table: Assembly Serial Details

Table: ICASENS
View: IC0167
Record length: 156
Flags: A R

## Keys: 3

Title | Flags | Fields
--- | --- | ---
Sequence/Comp/Parent Comp/Serial |  | ASSMENSEQ, COMPID, PRNCOMPID, SERIALNUMF
Sequence/Parent Comp/Comp/Serial |  | ASSMENSEQ, PRNCOMPID, COMPID, SERIALNUMF
Master Item Serial Number | M | ASSMENSEQ, PRNSERNUMF, COMPID, SERIALNUMF

## Fields: 12

Field | Type | Title | Presentation
--- | --- | --- | ---
ASSMENSEQ | Long | Sequence Number |
COMPID | Long | Component ID |
PRNCOMPID | Long | Parent Component ID |
SERIALNUMF | String*40 | Serial Number |
AUDTDATE | Date |  |
AUDTTIME | Time |  |
AUDTUSER | String*8 |  |
AUDTORG | String*6 |  |
PRNSERNUMF | String*40 | Master Item Serial Number |
ITEMNO | String*24 | Item Number | Mask: %-24C
BOMNO | String*6 | BOM Number | Mask: %-6N
UNIT | String*10 | Unit of Measure |

This page was generated on 2009-Nov-19

Copyright © 2001–2009 Sage Software, Inc. All rights reserved.